The cargo doors of the closed vehicles or closed containers shall be marked with the following in letters not less than 25 mm high:

            "WARNING
         NO VENTILATION
       OPEN WITH CAUTION"

This shall be in a language considered appropriate by the consignor.