This substance is classified as a flammable solid according to Appendix VI of Regulation (EC) No 1272/2008 (CLP Regulation). Because BAM does not have any data for a more precise assessment, the less favourable case (worst case) was assumed here, and packing group II was recommended. If appropriate classification data are available to the user, classification in packing group III may also be possible.