The following combination packagings are authorized, provided that the general provisions of 4.1.1 and 4.1.3 are met:

+---------------+--------------------------+----------+
| Inner         |                          | Maximum  |
| packagings    | Outer packagings         | net mass |
+---------------+--------------------------+----------+
| glass     5 l | Boxes                    |          |
| plastics  5 l |   aluminium (4B)         |  125 kg  |
| metal     5 l |   natural wood,          |  125 kg  |
|               |     ordinary (4C1)       |          |
|               |   natural wood, sift-    |  125 kg  |
|               |     proof walls (4C2)    |          |
|               |   plywood (4D)           |  125 kg  |
|               |   fibreboard (4G)        |  125 kg  |
|               |   plastics, solid (4H2)  |  125 kg  |
|               | Drums                    |          |
|               |   aluminium, removable   |  125 kg  |
|               |     head (1A1)           |          |
|               |   fibre (1G)             |  125 kg  |
|               |   other metal, removable |  125 kg  |
|               |     head (1N2)           |          |
|               |  plastics, removable     |  125 kg  |
|               |     head (1H2)           |          |
|               |   plywood (1D)           |  125 kg  |
|               | Jerricans                |          |
|               |   aluminium, removable   |  125 kg  |
|               |     head (3B2)           |          |
|               |   plastics, removable    |  125 kg  |
|               |     head (3H2)           |          |
+---------------+--------------------------+----------+