For the carriage of packages containing polymerizing substances the provisions of special provision 386, in conjunction with 7.1.7.3, 7.1.7.4, 5.4.1.1.15 and 5.4.1.2.3.1, need not be applied, when carried for disposal or recycling provided the following conditions are met:

(a) Before loading an examination has shown that there is no significant deviation between the outside temperature of the package and the ambient temperature;

(b) The carriage is effected within a period of not more than 24 hours from that examination;

(c) The packages are protected from direct sunlight and from the impact of other sources of heat (e.g. additional loads that are being carried above ambient temperature) during carriage;

(d) The ambient temperatures during the carriage are below 45 °C;

(e) Vehicles and containers are adequately ventilated; 

(f) The substances are packed in packages with a maximum capacity of 1000 litres.

In assessing the substances for carriage under the conditions of this special provision, additional measures to prevent dangerous polymerization may be considered, for example the addition of inhibitors.