When chemical stabilization is employed, the person offering the packaging for transport must ensure that the level of stabilization is sufficient to prevent the substance in the packaging from dangerous polymerization at a bulk mean temperature of 50 °C. Where chemical stabilization becomes ineffective at lower temperatures within the anticipated duration of transport, temperature control is required in which case the substances are forbidden for transport by air.