Packing Instruction 370

Passenger and cargo aircraft for UN 3269 (Packing Group II or III) only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

- Metal packagings must be corrosion resistant or be protected against corrosion for substances with a Class 8 subsidiary hazard.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

------------------------------------------------------------------------
                     COMBINATION PACKAGINGS
------------------------------------------------------------------------
           |            | Inner      |            |            |
           |            | packaging  | Inner      |Inner       |
           |            | quantity   | packaging  | packaging  |
           |            | (per       | quantity   | quantity   |
           |            | receptacle)| (per       | (per       |  Total
           |   Inner    | for liquid | receptacle)| receptacle)|quantity
 Packing   | packaging  | base       |- for liquid|- for solid |  per
 conditions| (see 6;3.2)| material   |  activator |  activator | package
------------------------------------------------------------------------
 Activator | Plastics*  |    n/a     |  125 mL    |   500 g    |
 (Organic  | --------------------------------------------------|
 peroxide) |  Metal     |    n/a     |  125 mL    |   500 g    |
---------------------------------------------------------------|
 Base      |  Glass     |   1.0 L    |   n/a      |    n/a     |  5 kg
 material  |---------------------------------------------------|
 Class 3   | Plastics   |   5.0 L    |   n/a      |    n/a     |
 Packing   |---------------------------------------------------|
 Group II  |  Metal     |   5.0 L    |   n/a      |    n/a     |
------------------------------------------------------------------------
 Activator | Plastics*  |    n/a     |  125 mL    |   500 g    |
 (Organic  | --------------------------------------------------|
 peroxide) |  Metal     |    n/a     |  125 mL    |   500 g    |
---------------------------------------------------------------|
 Base      |  Glass     |   2.5 L    |   n/a      |    n/a     | 10 kg
 material  |---------------------------------------------------|
 Class 3   | Plastics   |  10.0 L    |   n/a      |    n/a     |
 Packing   |---------------------------------------------------|
 Group III |  Metal     |  10.0 L    |   n/a      |    n/a     |
------------------------------------------------------------------------
*Including tubes

The total quantity of kits per package is to be calculated on a one-to-one basis
of their volume, i.e. 1 L equal to 1 kg.
-----------------------------------------------------------------------------------
 
ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

The components may be placed in the same outer packaging provided that they will not interact dangerously in the event of leakage (see 4;1.1.7).

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                       Drums                      Jerricans

Aluminium (4B)              Aluminium (1B1, 1B2)       Aluminium (3B1, 3B2)
Fibreboard (4G)             Fibre (1G)                 Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)     Other metal (1N1, 1N2)     Steel (3A1, 3A2)
Other metal (4N)            Plastics (1H1, 1H2)
Plastics (4H1, 4H2)         Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)