Packing Instruction 964 (for UN 1990)

Passenger and cargo aircraft for UN 1990 only

General requirements

Part 4, Chapter 1 requirements must be met. These requirements include:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

------------------------------------------------------------------
                       COMBINATION PACKAGINGS 
------------------------------------------------------------------
                         |         |Inner      |Total    |Total
                         |  Inner  |packaging  |quantity |quantity
                         |packaging|quantity   |  per    |  per
UN number and proper     |  (see   | (per      |package -|package-
shipping name            |  6;3.2) |receptacle)|passenger| cargo
------------------------------------------------------------------
UN 1990 Benzaldehyde     |  Glass  |  10.0 L   |         |
                         |---------------------|         |
                         | Plastics|  30.0 L   |  100 L  | 220 L
                         |---------------------|         |
                         |  Metal  |  40.0 L   |         |
------------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                        Drums                     Jerricans

Aluminium (4B)               Aluminium (1B1, 1B2)      Aluminium (3B1, 3B2)
Fibreboard (4G)              Fibre (1G)                Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)      Other metal (1N1, 1N2)    Steel (3A1, 3A2)
Other metal (4N)             Plastics (1H1, 1H2)            
Plastics (4H1, 4H2)          Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)