Verpackungsanweisung 472

Passenger and cargo aircraft für UN 1362 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

----------------------------------------------------------------------
                   COMBINATION PACKAGINGS
----------------------------------------------------------------------
                          |Inner      |Inner packaging |
UN number and proper      |packaging  |quantity (per   |Total quantity
shipping name             |(see 6;3.2)|receptacle)     |per package
----------------------------------------------------------------------
UN 1362 Carbon, activated |  Plastics |     0.1 kg     |    0.5 kg
----------------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                           Drums                        Jerricans

Aluminium (4B)                  Aluminium (1B1, 1B2)         Aluminium (3B1, 3B2)
Steel (4A)                      Steel (1A1, 1A2)             Steel (3A1, 3A2)