Verpackungsanweisung 217 (für UN 3478)

Passenger and cargo aircraft for UN 3478 (packed with equipment) only

General requirements

Part 4;1.1.1 and 1.1.7 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

--------------------------------------------------------------------------------
UN number and proper shipping name   |      Quantity -     |       Quantity -
                                     |      passenger      |        cargo
--------------------------------------------------------------------------------
UN3478 Fuel cell cartridges          | 1 kg of fuel cell   |  15 kg of fuel cell
packed with equipment,               |     cartridges      |      cartridges
containing liquefied flammable gas   |                     |
--------------------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS

- When fuel cell cartridges are packed with equipment, they must be packed in intermediate packagings together with the equipment they are capable of powering.

- The maximum number of fuel cell cartridges in the intermediate packaging must be the minimum number required to power the equipment, plus 2 spares.

- The fuel cell cartridges and the equipment must be packed with cushioning material or divider(s) or inner packaging so that the fuel cell cartridges are protected against damage that may be caused by the movement or placement of the equipment and the cartridges within the packaging.

OUTER PACKAGINGS

Boxes                        Drums                        Jerricans

                     Strong outer packagings