Verpackungsanweisung 473 (für UN 2881 PG III)

Passenger and cargo aircraft - for UN 2881 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

-------------------------------------------------------------------
                        COMBINATION PACKAGINGS
-------------------------------------------------------------------
          |     |       |  Inner    |         |Inner      |
          |     |Inner  | packaging |Total    |packaging  |Total
UN number |     |packa- |quantity   |quantity |quantity   |quantity
and proper|Pack-|ging   |   (per    | per     |(per       |per
shipping  | ing |(see   |receptacle)|package -|receptacle)|package
 name     |group|6;3.2) |- passenger|passenger| - cargo   |- cargo
-------------------------------------------------------------------
UN 2881   |     | Glass |   1.0 kg  |  25 kg  |  2.5 kg   | 100 kg
 Metal    | III |--------------------------------------------------
 catalyst,|     | Metal |   1.0 kg  |  25 kg  |  5.0 kg   | 100 kg
 dry      |     |       |                     |           |
-------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

Packing Group III

- Packagings must meet the Packing Group II performance requirements.

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                       Drums                       Jerricans
  
Aluminium (4B)              Aluminium (1B1, 1B2)        Aluminium (3B1, 3B2)
Fibreboard (4G)             Fibre (1G)                  Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)     Other metal (1N1, 1N2)      Steel (3A1, 3A2)
Other metal (4N)            Plastics (1H1, 1H2)
Plastics (4H1, 4H2)         Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)