Packing Instruction 971 (for UN 3508)

Passenger and cargo aircraft for UN 3508 (Special Provision A196) only

General requirements

Part 4;1.1.1 and 1.1.8 requirements must be met.

For the purpose of this packing instruction, a capacitor is considered an inner packaging.

-------------------------------------------------------------------------------
UN number and                 |                        |  
proper shipping name          | Quantity - passenger   | Quantity - cargo
-------------------------------------------------------------------------------
UN 3508 Capacitor, asymmetric |                        |
        (with an energy       |                        |
        storage capacity      |       No limit         |       No limit
        greater than 0.3Wh)   |                        |
-------------------------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                        Drums                        Jerricans
                     Strong outer packagings