Verpackungsanweisung 873

Passenger and cargo aircraft für UN 3477

General requirements

Part 4;1.1.1, 1.1.2 and 1.1.7 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

-----------------------------------------------------------------------------------
UN number and proper shipping name   |    Quantity -     |         Quantity -
                                     |    passenger      |           cargo
-----------------------------------------------------------------------------------
UN 3477 Fuel cell cartridges         |5 kg of fuel cell  |  50 kg of fuel cell
                                     |    cartridges     |       cartridges
-----------------------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS

- Fuel cell cartridges must be securely cushioned in the outer packagings.

- The mass of each fuel cell cartridge must not exceed 1 kg.

- Packagings must meet the Packing Group II performance requirements.
           
OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                        Drums                        Jerricans

Aluminium (4B)               Aluminium (1B2)              Steel (3A2)
Fibreboard (4G)              Fibreboard (1G)              Plastics (3H2)
Natural wood (4C1, 4C2)      Plastics (1H2)                Aluminium (3B2)
Other metal (4N)             Plywood (1D)
Plastics (4H2)               Steel (1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)