Packing Instruction 497

Passenger and cargo aircraft for UN 3476 (packed with equipment) only

General requirements

Part 4;1.1.1 and 1.1.7 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

-----------------------------------------------------------------------------------
UN number and proper shipping name |      Quantity -    |          Quantity -
                                   |      passenger     |            cargo
-----------------------------------------------------------------------------------
UN3476 Fuel cell cartridges        | 5 kg of fuel cell  |   50 kg of fuel cell
       packed with equipment       |     cartridges     |        cartridges
-----------------------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS

- When fuel cell cartridges are packed with equipment, they must be packed in intermediate packagings together with the equipment they are capable of powering.

- The maximum number of fuel cell cartridges in the intermediate packaging must be the minimum number required to power the equipment, plus two spares.

- The fuel cell cartridges and the equipment must be packed with cushioning material or divider(s) or inner packaging so that the fuel cell cartridges are protected against damage that may be caused by the movement or placement of the equipment and the cartridges within the packaging.

- The mass of each fuel cell cartridge must not exceed 1 kg.

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                        Drums                        Jerricans

                     Strong outer packagings