In accordance with Part 2, Introductory Chapter, paragraph 4, this radioactive material in an excepted package possessing toxic and corrosive properties is classified in Division 6.1 with radioactive and corrosive subsidiary hazard.

Uranium hexafluoride may be classified under this entry only if the conditions of 2;7.2.4.1.1.2, 2;7.2.4.1.1.5, 2;7.2.4.5.2 and, for fissile-excepted material, of 2;7.2.3.6 are met.

In addition to the provisions applicable to the transport of Division 6.1 substanceswith a corrosive subsidary hazard, the provisions of 5;1.2.2.2, 5;1.6.3, 7;1.6 and 7;3.2.1 to 7;3.2.4 apply.

No Class 7 label is required to be displayed.