When the shaped charges are packed singly, the conical cavity must face downwards and the package must be marked as illustrated in Figure 5-29. When the shaped charges are packed in pairs, the conical cavities must face inwards to minimize the jetting effect in the event of accidental initiation.