Combination packagings are allowed.

Part 4, Chapter 1 requirements must be met.

Single packagings are not allowed.

Note: Solids having an inhalation toxicity of Packing Group I are forbidden on passenger aircraft.