N_CODE	S_ANHAFTENDE_GEFAHR	S_RISIKO_FLUGZEUG	S_RISIKO_INSASSEN	S_PROZEDUR_LECK	S_PROZEDUR_FEUER	S_ZUS_BETRACHTUNGEN	S_SPRACHE
1	Explosion may cause structural failure	Fire and/or explosion	As indicated by the drill letter(s)	Use 100 % oxygen; no smoking	All agents according to availability; use standard fire procedure	Possible abrupt loss of pressurization	E
2	Gas, non-flammable, pressure may create hazard in fire	Minimal	As indicated by the drill letter(s)	Use 100 % oxygen; establish and maintain maximum ventilation for "A", "i" or "P" drill letter	All agents according to availability; use standard fire procedure	Possible abrupt loss of pressurization	E
3	Flammable liquid or solid	Fire and/or explosion	Smoke, fumes and heat, and as indicated by the drill letter(s)	Use 100 % oxygen; establish and maintain maximum ventilation; no smoking; minimum electrics	All agents according to availability; no water on "W" drill letter	Possible abrupt loss of pressurization	E
4	Spontaneously combustible or pyrophoric when exposed to air	Fire and/or explosion	Smoke, fumes and heat, and as indicated by the drill letter(s)	Use 100 % oxygen; establish and maintain maximum ventilation	All agents according to availability; no water on "W" drill letter	Possible abrupt loss of pressurization; minimum electrics if "F" or "H" drill letter	E
5	Oxidizer, may ignite other materials, may explode in heat of a fire	Fire and/or explosion, possible corrosion damage	Eye, nose and throat irritation; skin damage on contact	Use 100 % oxygen; establish and maintain maximum ventilation	All agents according to availability; no water on "W" drill letter	Possible abrupt loss of pressurization	E
6	Toxic, may be fatal if inhaled, ingested, or absorbed by skin	Contamination with toxic liquid or solid	Acute toxicity, effects may be delayed	Use 100 % oxygen; establish and maintain maximum ventilation; do not touch without gloves	All agents according to availability; no water on "W" drill letter	Possible abrupt loss of pressurization; minimum electrics if "F" or "H" drill letter	E
8	Corrosive, fumes disabling if inhaled or in contact with skin	Possible corrosion damage	Eye, nose and throat irritation; skin damage on contact	Use 100 % oxygen; establish and maintain maximum ventilation; do not touch without gloves	All agents according to availability; no water on "W" drill letter	Possible abrupt loss of pressurization; minimum electrics if "F" or "H" drill letter	E
9	No general inherent hazard	As indicated by the drill letter	As indicated by the drill letter	Use 100 % oxygen; establish and maintain maximum ventilation if "A" drill letter	All agents according to availability	None	E
10	Gas, flammable, high fire risk if any ignition source present	Fire and/or explosion	Smoke, fumes and heat and as indicated by the drill letter(s)	Use 100 % oxygen; establish and maintain maximum ventilation; no smoking; minimum electrics	All agents according to availability	Possible abrupt loss of pressurization	E
11	Infectious substances may affect humans or animals if inhaled, ingested or absorbed through the mucous membrane or an open wound	Contamination with Infectious substances	Delayed infection to humans or animals	Do not touch. Minimum recirculation and ventilation in affected area.	All agents according to availability. No water on 'Y' drill letter	Call for a qualified person to meet the aircraft	E
12	Fire, heat, smoke, toxic and flammable vapour	Fire and/or explosion	Smoke, fumes, heat	Use 100% oxygen; establish and maintain maximum ventilation	All agents according to availability. Use water if available	Possible abrupt loss of pressurization; consider landing immediately	E
