Packing Instruction 374

Passenger and cargo aircraft for UN 3473 only

General requirements

Part 4;1.1.1, 1.1.2 and 1.1.7 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

-----------------------------------------------------------------------------------
UN number and proper shipping name |      Quantity -    |          Quantity -
                                   |      passenger     |            cargo
----------------------------------------------------------------------------------- 
UN3473 Fuel cell cartridges        | 5 kg of fuel cell  |  50 kg of fuel cell
                                   |      cartridges    |        cartridges
-----------------------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS

- Fuel cell cartridges must be securely cushioned in the outer packagings.
- Packagings must meet the Packing Group II performance requirements.
           
OUTER PACKAGINGS

Boxes                        Drums                        Jerricans

Aluminium (4B)               Aluminium (1B2)              Steel (3A2)
Fibreboard (4G)              Fibreboard (1G)              Plastics(3H2)
Natural wood (4C1, 4C2)      Plastics (1H2)               Aluminium (3B2)
Other metal (4N)             Plywood (1D)
Plastics (4H1, 4H2)          Steel (1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)