Verpackungsanweisung 454

Passenger and cargo aircraft für UN 1324 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

---------------------------------------------------------------------
COMBINATION PACKAGINGS
---------------------------------------------------------------------
UN number and proper               | Total quantity | Total quantity
shipping name                      | per package -  | per package -
                                   |   passenger    |    cargo
---------------------------------------------------------------------
UN 1324 Films, nitrocellulose base |     25 kg      |     100 kg
---------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

- Packagings must meet the Packing Group II performance requirements.

- Each reel must be placed in a tightly closed metal can or strong cardboard or fibreboard inner packaging with cover held in place by adhesive tape or paper.

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                           Drums                    Jerricans

Aluminium (4B)                  Aluminium (1B1, 1B2)     Aluminium (3B1, 3B2)
Fibreboard (4G)*                Fibre (1G)*              Plastics (3H1, 3H2)*
Natural wood (4C1, 4C2)         Other metal (1N1, 1N2)   Steel (3A1, 3A2)
Other metal (4N)                Plastics (1H1, 1H2)*
Plastics (4H1, 4H2)*            Plywood (1D)
Plywood (4D)                    Steel (1A1, 1A2)
Reconstituted wood (4F)
Steel (4A)

* These packagings are permitted only for a maximum of 600 m of film.