Packing Instruction 473 (for UN 1378)

Passenger and cargo aircraft - for UN 1378 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

-------------------------------------------------------------------
                        COMBINATION PACKAGINGS
-------------------------------------------------------------------
          |     |       |  Inner    |         |Inner      |
          |     |Inner  | packaging |Total    |packaging  |Total
UN number |     |packa- |quantity   |quantity |quantity   |quantity
and proper|Pack-|ging   |   (per    | per     |(per       |per
shipping  | ing |(see   |receptacle)|package -|receptacle)|package
 name     |group|6;3.2) |- passenger|passenger| - cargo   |- cargo
-------------------------------------------------------------------
UN 1378   |     | Glass |                     |  1.0 kg   |
 Metal    |  II |-------|       Forbidden     |-----------| 50 kg
 catalyst,|     | Metal |                     |  1.0 kg   |
 wetted   |     |       |                     |           |
-------------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                       Drums                       Jerricans
  
Aluminium (4B)              Aluminium (1B1, 1B2)        Aluminium (3B1, 3B2)
Fibreboard (4G)             Fibre (1G)                  Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)     Other metal (1N1, 1N2)      Steel (3A1, 3A2)
Other metal (4N)            Plastics (1H1, 1H2)
Plastics (4H1, 4H2)         Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)