Verpackungsanweisung 459 (für UN 3228)

Passenger and cargo aircraft - self-reactive substances and polymerizing substances

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements
   
- Substances must be compatible with their packagings as required by 4;1.1.3.
   
2) Closure requirements
   
- Closures must meet the requirements of 4;1.1.4.

--------------------------------------------------------------------------
COMBINATION PACKAGINGS
--------------------------------------------------------------------------
                     |         |Inner      |         |Inner      |
                     |         |packaging  |Total    |packaging  |Total
                     |Inner    |quantity   |quantity |quantity   |quantity
                     |packaging|(per       |per      |(per       |per
UN number and proper |(see     |receptacle)|package -|receptacle)|package
shipping name        |6;3.2)   |- passenger|passenger|- cargo    |- cargo
--------------------------------------------------------------------------
Solids
--------------------------------------------------------------------------
UN 3228 Self-reactive| Plastic |   1.0 kg  | 10 kg   |   2.5 kg  |  25 kg
        solid type E | ---------------------------------------------------
                     | Plastic |           |         |           |
                     | bag     |   1.0 kg  | 10 kg   |   2.5 kg  |  25 kg
--------------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

- Cushioning materials must not be readily combustible.

- Packagings must meet the Packing Group II performance requirements.

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                        Drums                Jerricans

Fibreboard (4G)              Fibre (1G)           Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)      Plastics (1H1, 1H2)      
Plastics (4H1, 4H2)          Plywood (1D)
Plywood (4D)                 
Reconstituted wood (4F)