The construction materials of the cylinders and their accessories must be compatible with the contents and must not react to form harmful or dangerous compounds therewith.

The test pressure and filling ratio must be calculated in accordance with the relevant requirements of PI 200.

The necessary steps must be taken to prevent dangerous reactions (i.e. polymerization or decomposition) during transport. If necessary, stabilization or addition of an inhibitor may be required.