Verpackungsanweisung 957 (für UN 3314)

Passenger and cargo aircraft for  UN 3314 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.
------------------------------------------------------------------------
                     COMBINATION PACKAGINGS
------------------------------------------------------------------------
                         |             | Inner      |          |
                         |             | packaging  |          |
                         | Inner       | quantity   |          |
 UN number and proper    | packaging   | (per       |Quantity -|Quantity
 shipping name           | (see 6;3.2) | receptacle)|passenger |- cargo
------------------------------------------------------------------------
UN 2211 Plastics         |   Glass     |   10 kg    |  100 kg  | 200 kg
        moulding         |--------------------------|          |
        compound in      |   Fibre     |   50 kg    |          |
        dough, sheet or  |--------------------------|          |
        extruded rope    |    Metal    |   50 kg    |          |
        form evolving    |--------------------------|          |
        flammable vapour |  Paper bag  |   50 kg    |          |
                         |--------------------------|          |
                         |  Plastics   |   50 kg    |          |
                         |--------------------------|          |
                         | Plastic bag |   50 kg    |          |
------------------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                         Drums                      Jerricans

Aluminium (4B)                Aluminium (1B1, 1B2)       Aluminium (3B1, 3B2)
Fibreboard (4G)               Fibre (1G)                 Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)       Other metal (1N1, 1N2)     Steel (3A1, 3A2)
Other metal (4N)              Plastics (1H1, 1H2)
Plastics (4H1, 4H2)           Plywood (1D)
Plywood (4D)                  Steel (1A1, 1A2)
Reconstituted wood (4F)
Steel (4A)