Packing Instruction 864 (only soft packaging)

Cargo aircraft only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

- Substances of Class 8 are permitted in glass or earthenware inner packagings only if the substance is free from hydrofluoric acid.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

---------------------------------------------------------------------
                      COMBINATION PACKAGINGS
---------------------------------------------------------------------
            |         | Inner      | Inner packaging|
  Packing   | Packing | packaging  | quantity (per  | Total quantity
instruction |  group  | (see 6;3.2)| receptacle)    | per package
---------------------------------------------------------------------
            |         |  Plastics  |     5.0 kg     |
    864     |   III   |-----------------------------|   100 kg
            |         |Plastic bag |     5.0 kg     |
---------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

Packing Group III

- Packagings must meet the Packing Group II performance requirements.

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                         Drums                      Jerricans

Fibreboard (4G)               Fibre (1G)                 Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)       Plastics (1H1, 1H2)
Plastics (4H1, 4H2)           Plywood (1D)
Plywood (4D)
Reconstituted wood (4F)