Packing Instruction 852  (only soft packaging)

Passenger aircraft

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

- Substances of Class 8 are permitted in glass or earthenware inner packagings only if the substance is free from hydrofluoric acid.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

---------------------------------------------------------------------
                      COMBINATION PACKAGINGS
---------------------------------------------------------------------
            |         | Inner      | Inner packaging|
  Packing   | Packing | packaging  | quantity (per  | Total quantity
instruction |  group  | (see 6;3.2)| receptacle)    | per package
---------------------------------------------------------------------
    852     |   III   |  Plastics  |     2.5 L      |      5 L
---------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

Packing Group III

- Packagings must meet the Packing Group II performance requirements.

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                     Drums                     Jerricans

Fibreboard (4G)           Fibre (1G)                Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)   Plastics (1H1, 1H2)
Plastics (4H1, 4H2)
Plywood (4D)
Reconstituted wood (4F)