Mixtures of solids which are not subject to these Instructions and corrosive liquids may be transported under this entry without first applying the classification criteria of Class 8, providing there is no free liquid visible at the time the substance is packaged and, for single packagings, the packaging must pass a leakproofness test at the packing group II level.