See remarks 13), 16) and 19) to Table 2-7:

13) "CORROSIVE" subsidiary hazard label required (see Figure 5-24).

16) Peroxyacetic acid formulations which fulfil the criteria of 2;5.3.2.4.

19) Mixtures with hydrogen peroxide, water and acid(s).