Mixtures of nitrogen and oxygen containing not less than 19.5 per cent and not more than 23.5 per cent oxygen by volume may be transported under this entry when no other oxidizing gases are present. A Division 5.1 subsidiary hazard label is not required for any concentrations within this limit.