In the ERG Code of the ICAO TI, the ERG code for the variant with a solid base product (UN 3527) is "3S", whereas the ERG code for the variant with a liquid base product (UN 3269) is "3L". The drill letter "S" for "Spontaneously compostible or pyrophoric" may be too strict.