Packing Instruction 681 (for UN 3362)

Cargo aircraft only for Chlorosilanes

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

- Metal packagings must be corrosion resistant or be protected against corrosion.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

------------------------------------------------------------------
                      COMBINATION PACKAGINGS
------------------------------------------------------------------
                 |  Inner       | Net quantity   |
                 |  packaging   | per inner      | Total quantity
 UN number       |  (see 6;3.2) | packaging      | per package
------------------------------------------------------------------
                 |   Glass      |     1.0 L      |
 UN 3362         |-------------------------------|
                 |  Plastics    |   Forbidden    |    30.0 L
                 |-------------------------------|
                 |   Steel      |     1.0 L      |
------------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS

Boxes                                 Drums

Fibreboard (4G)                       Fibre (1G)
Natural wood (4C1, 4C2)               Plastics (1H1, 1H2)
Plastics (4H1, 4H2)                   Plywood (1D)
Plywood (4D)                          Steel (1A1, 1A2)
Reconstituted wood (4F)
Steel (4A)