Packing Instruction 871

Passenger and cargo aircraft for UN 3028 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

- Metal packagings must be corrosion resistant or be protected against corrosion.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

-----------------------------------------------------------------------
                  |                                 | Total   |  Total
                  |                                 | quantity|quantity
UN number and     |                                 |  per    |  per
proper            |                                 |package -|package
shipping name     | Packing conditions              |passenger|- cargo
-----------------------------------------------------------------------
UN 3028 Batteries,|The batteries must be securely   |         |
   dry, containing|cushioned in the packagings.     | 25 kg   | 230 kg
   potassium      |                                 |         |
   hydroxide solid|                                 |         |
-----------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS

- Packagings must meet the Packing Group II performance requirements.

PACKAGINGS

Boxes

Aluminium (4B))
Fibreboard (4G)
Natural wood (4C1, 4C2)
Plastics (4H2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)