Verpackungsanweisung 956 (für UN 3077)

Passenger and cargo aircraft for UN 3077 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

---------------------------------------------------------------
                       COMBINATION PACKAGINGS
---------------------------------------------------------------
                    |           |Inner      |Total    |Total
                    |   Inner   |packaging  |quantity |quantity
                    | packaging |quantity   |  per    |  per
UN number and proper|  (see     | (per      |package -|package
shipping name       |   6;3.2)  |receptacle)|passenger|- cargo
---------------------------------------------------------------
UN 3077 Environmen- |   Glass   |  10.0 kg  |         |
   tally hazardous  |-----------------------|         |
   substance, solid,|   Fibre   |  50.0 kg  |         |
   n.o.s.           |-----------------------|         |
                    |   Metal   |  50.0 kg  |         |
                    |-----------------------| 400 kg  | 400 kg
                    | Paper bag |  50.0 kg  |         |
                    |-----------------------|         |
                    |  Plastics |  50.0 kg  |         |
                    |-----------------------|         |
                    |Plastic bag|  50.0 kg  |         |
---------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                       Drums                          Jerricans

Aluminium (4B)              Aluminium (1B1, 1B2)           Aluminium (3B1, 3B2)
Fibreboard (4G)             Fibre (1G)                     Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)     Other metal (1N1, 1N2)         Steel (3A1, 3A2)
Other metal (4N)            Plastics (1H1, 1H2)
Plastics (4H1, 4H2)         Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)