Note by BAM: in the ICAO Technical Instructions this peroxide is contrary to the UN Model Regulations (there diluent type B) with the entry diluent type A. Because diluent type B is stated in the UN Model Regulations, it is assumed that diluent type B is meant here.