Packing Instruction 570 (for UN 3105)

Passenger and cargo aircraft

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.
   
2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

--------------------------------------------------------------------------
                            COMBINATION PACKAGINGS
--------------------------------------------------------------------------
                     |         |Inner      |         |Inner      |
                     |         |packaging  |Total    |packaging  |Total
                     |Inner    |quantity   |quantity |quantity   |quantity
                     |packaging|(per       |per      |(per       |per
UN number and proper |(see     |receptacle)|package -|receptacle)|package
shipping name        |6;3.2)   |- passenger|passenger|- cargo    |- cargo
--------------------------------------------------------------------------
Liquids
--------------------------------------------------------------------------
UN 3105 Organic per- |         |           |         |           |
        oxide type D,| Plastics|   0.5 L   |  5 L    |   1.0 L   |  10 L
        liquid       |         |           |         |           |
--------------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

- Packagings must meet the Packing Group II performance requirements.

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                          Drums                       Jerricans

Fibreboard (4G)                Fibre (1G)                  Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)        Plastics (1H1, 1H2)
Plastics (4H1, 4H2)            Plywood (1D)
Plywood (4D)
Reconstituted wood (4F)