Packing Instruction 956 (for UN 3152)

Passenger and cargo aircraft for UN 3152 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

---------------------------------------------------------------
                       COMBINATION PACKAGINGS
---------------------------------------------------------------
                    |           |Inner      |Total    |Total
                    |   Inner   |packaging  |quantity |quantity
                    | packaging |quantity   |  per    |  per
UN number and proper|  (see     | (per      |package -|package
shipping name       |   6;3.2)  |receptacle)|passenger|- cargo
---------------------------------------------------------------
UN 3152 Polyhaloge- |   Glass   |  10.0 kg  |         |
   nated biphenyls, |-----------------------|         |
   solid or Polyha- |   Fibre   |  50.0 kg  |         |
   logenated        |-----------------------|         |
   terphenyls, solid|   Metal   |  50.0 kg  |         |
   or Halogenated   |-----------------------| 100 kg  | 200 kg
   monomethyl-      | Paper bag |  50.0 kg  |         |
   diphenylmethanes,|-----------------------|         |
   solid            |  Plastics |  50.0 kg  |         |
                    |-----------------------|         |
                    |Plastic bag|  50.0 kg  |         |
---------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                       Drums                          Jerricans

Aluminium (4B)              Aluminium (1B1, 1B2)           Aluminium (3B1, 3B2)
Fibreboard (4G)             Fibre (1G)                     Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)     Other metal (1N1, 1N2)         Steel (3A1, 3A2)
Other metal (4N)            Plastics (1H1, 1H2)
Plastics (4H1, 4H2)         Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)