Mixtures of solids which are not subject to these Instructions and toxic liquids may be transported under this entry without first applying the classification criteria of Division 6.1, providing there is no free liquid visible at the time the substance is packaged and, for single packagings, the packaging must pass a leakproofnesstest at the packing group II level. This entry must not be used for solids containing a Packing Group I liquid.