For magnetized materials the special provisions of Packing Instruction 953 apply.

Für Magnetisches Material gelten besondere Bestimmungen -
siehe Verpackungsanweisung (Packing Instruction) 953.

Passenger and cargo aircraft for UN 2807 only

--------------------------------------------------------------------------
                                             | Quantity -  | Quantity -
UN number and proper shipping name           | passenger   |   cargo
--------------------------------------------------------------------------
UN 2807 Magnetized material                  |  No limit   |  No limit
--------------------------------------------------------------------------

Magnetized materials with field strengths causing a compass deflection of more than 2 degrees at a distance of 2.1 m but not more than 2 degrees at a distance of 4.6 m (equivalent to 0.418 A/m or 0.00525 Gauss measured at a distance of 4.6 m) are not subject to any other requirements in these Instructions when carried as cargo except for the following:

a) The shipper must make prior arrangements with the operator identifying the magnetized material. The dangerous goods transport document requirements of Part 5;4 are not applicable provided alternative written or electronic documentation includes the words "magnetized material" in association with the description of the goods;

b) The package must bear the magnetized material handling label;

c) The operator must stow the packaged magnetized material in accordance with 7;2.10; and

d) The incident reporting requirements of 7;4.4 must be met.

Magnetized material with field strength sufficient to cause a compass deflection of more than 2 degrees at a distance of 4.6 m may only be transported with the prior approval of the appropriate authority of the State of Origin and the State of the Operator.