Packing Instruction 956 (for UN 3432)

Passenger and cargo aircraft for UN 3432 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

---------------------------------------------------------------
                       COMBINATION PACKAGINGS
---------------------------------------------------------------
                    |           |Inner      |Total    |Total
                    |   Inner   |packaging  |quantity |quantity
                    | packaging |quantity   |  per    |  per
UN number and proper|  (see     | (per      |package -|package
shipping name       |   6;3.2)  |receptacle)|passenger|- cargo
---------------------------------------------------------------
UN 3432 Polychlori- |   Glass   |  10.0 kg  |         |
   nated biphenyls, |-----------------------|         |
   solid            |   Fibre   |  50.0 kg  |         |
                    |-----------------------|         |
                    |   Metal   |  50.0 kg  |         |
                    |-----------------------| 100 kg  | 200 kg
                    | Paper bag |  50.0 kg  |         |
                    |-----------------------|         |
                    |  Plastics |  50.0 kg  |         |
                    |-----------------------|         |
                    |Plastic bag|  50.0 kg  |         |
---------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                       Drums                          Jerricans

Aluminium (4B)              Aluminium (1B1, 1B2)           Aluminium (3B1, 3B2)
Fibreboard (4G)             Fibre (1G)                     Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)     Other metal (1N1, 1N2)         Steel (3A1, 3A2)
Other metal (4N)            Plastics (1H1, 1H2)
Plastics (4H1, 4H2)         Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)