Verpackungsanweisung 866

Cargo aircraft only for UN 2028 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

- Metal packagings must be corrosion resistant or be protected against corrosion.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

----------------------------------------------------------------------------
                        COMBINATION PACKAGINGS
----------------------------------------------------------------------------
                       |                            |  Total    |  Total
UN number and          |                            | quantity  |  quantity
proper shipping        |                            |per package|per package
name                   |Packing conditions          |- passenger|  - cargo
----------------------------------------------------------------------------
UN 2028 Bombs, smoke,  |Bombs, smoke may be carried |           |
        non-explosive  |provided they are without   |           |
        with corrosive |ignition elements, bursting | Forbidden |   50 kg
        liquid, without|charges, detonating fuses or|           |
        initiating     |other explosive components. |           |
        device         |                            |           |
----------------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

- Packagings must meet the Packing Group II performance requirements.
- The articles must be individually packaged and separated from each other using partitions, dividers, inner packagings or cushioning material.

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                      Drums                   

Aluminium (4B)             Aluminium (1B2)
Fibreboard (4G)            Fibre (1G)
Natural wood (4C1, 4C2)    Other metal (1N2)
Other metal (4N)           Plastics (1H2)
Plastics (4H1, 4H2)        Steel (1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)