Phthalic anhydride in the solid state and tetrahydrophthalic anhydrides, with not more than 0.05 per cent maleic anhydride, are not subject to these Instructions. Phthalic anhydride molten at a temperature above its flash
point, with not more than 0.05 per cent maleic anhydride, must be classified under UN 3256.