Notwithstanding the Division 6.1 subsidiary hazard shown in column 4 of Table 3-1, the toxic subsidiary hazard label and an indication of this subsidiary hazard on the dangerous goods transport document are not required when the manufactured articles contain not more than 5 kg of mercury. Transport in accordance with this special provision must be noted on the dangerous goods transport document.