"Type C packages may be transported as air cargo if the activities of the radioactive material exceed 3000 A1 or 3000 A2.
For all other modes of transportation, Type B(U) and Type B(M) packages are sufficient."
