Packing Instruction 876 (for UN 1800)

Cargo aircraft only for Chlorosilanes

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

- Metal packagings must be corrosion resistant or be protected against corrosion.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

---------------------------------------------------------------
COMBINATION PACKAGINGS
---------------------------------------------------------------
                  |                   |Net quantity|    Total
                  |                   | per inner  |  quantity
                  |  Inner packaging  | packaging  |per package 
UN number         |    (see 6;3.2)    |  - cargo   |  - cargo
---------------------------------------------------------------
 UN 1800          |                   |            |
                  |       Glass       |   1.0 L    |
                  |                   |            |
                  |------------------------------- |
                  |                   |            |
                  |      Plastics     | Forbidden  |   30.0 L
                  |                   |            |
                  |--------------------------------|
                  |                   |            |
                  |       Steel       |   5.0 L    |
                  |                   |            |
                  |                   |            |
---------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS

Boxes                            Drums

Fibreboard (4G)                  Fibre (1G)
Natural wood (4C1, 4C2)          Plastics (1H1, 1H2)
Plastics (4H1, 4H2)              Plywood (1D)
Plywood (4D)                     Steel (1A1, 1A2)
Reconstituted wood (4F)
Steel (4A)