Verpackungsanweisung 680

Passenger and cargo aircraft für UN 1888 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

---------------------------------------------------------------------
                      COMBINATION PACKAGINGS
---------------------------------------------------------------------
                 |        | Inner     | Inner     |         |
                 | Inner  | packaging |packaging  |  Total  | Total
                 |packa-  | quantity  |quantity   |quantity |quantity
 UN number and   | ging   | (per      | (per      |  per    |  per
 proper          | (see   |receptacle)|receptacle)|package -|package
 shipping name   |6;3.2)  |- passenger|- cargo    |passenger|- cargo
---------------------------------------------------------------------
 UN 1888         | Glass  |   1.0 L   |  2.5 L    |         |
 Chloroform      |--------------------------------|         |
                 |Plastics|   1.0 L   |  2.5 L    |  60 L   | 220 L
                 |--------------------------------|         |
                 | Metal  |   2.5 L   |  5.0 L    |         |
---------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

- Inner packagings must be packed with sufficient absorbent material to absorb the entire contents of the inner packagings and placed in a rigid leakproof receptacle before packing in outer packagings.

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                      Drums                     Jerricans

Aluminium (4B)             Aluminium (1B2, 1B2)      Aluminium (3B1, 3B2)
Fibreboard (4G)            Fibre (1G)                Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)    Other metal (1N1, 1N2)    Steel (3A1, 3A2)
Other metal (4N)           Plastics (1H1, 1H2)
Plastics (4H1, 4H2)        Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)