Packing Instruction 964 (for UN 3082)

Passenger and cargo aircraft for UN 3082 only

General requirements

Part 4, Chapter 1 requirements must be met (with the exception that for UN 3082 packed in combination packagings, the requirements of 4;1.1.6 do not apply). These requirements include:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

------------------------------------------------------------------
                       COMBINATION PACKAGINGS 
------------------------------------------------------------------
                         |         |Inner      |Total    |Total
                         |  Inner  |packaging  |quantity |quantity
                         |packaging|quantity   |  per    |  per
UN number and proper     |  (see   | (per      |package -|package-
shipping name            |  6;3.2) |receptacle)|passenger| cargo
------------------------------------------------------------------
UN 3082 Environmentally  |  Glass  |  10.0 L   |         |
   hazardous substance,  |---------------------|         |
   liquid, n.o.s.        | Plastics|  30.0 L   |  450 L  | 450 L
                         |---------------------|         |
                         |  Metal  |  40.0 L   |         |
------------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                        Drums                     Jerricans

Aluminium (4B)               Aluminium (1B1, 1B2)      Aluminium (3B1, 3B2)
Fibreboard (4G)              Fibre (1G)                Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)      Other metal (1N1, 1N2)    Steel (3A1, 3A2)
Other metal (4N)             Plastics (1H1, 1H2)            
Plastics (4H1, 4H2)          Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)