Items classified as explosive must be removed from vehicles and transported in accordance with the provisions of these Instructions unless authorized by the appropriate national authority under the written conditions established by that authority. In such circumstances, vehicles may be transported on cargo aircraft only.

Note.- This Special Provision does not apply where the explosives are a smoke candle installed as a permanent pan of the vehicle or are part of an assembly classified as dangerous goods of other than Class 1, e.g. Air bag inflators, Air bag modules and Seat- belt pretensioners (UN 3268), Fire extinguishers (UN 1044), and Gas generator assemblies, (ID 8013). Additionally this Special Provision does not apply in the case of Air bag modules and Air bag inflators and Seat-belt pretensioners (UN 0503) installed in the vehicle.