Articles containing smoke-producing substance(s) corrosive according to the criteria for Class 8 must be labelled with a "Corrosive" subsidiary hazard label. Articles containing smoke-producing substance(s) toxic by inhalation according to the criteria for Division 6.1 must be labelled with a "TOXIC" subsidiary hazard label (Figure 5-18).