Verpackungsanweisung 964 (für UN 1941)

Passenger and cargo aircraft for UN 1941 only

General requirements

Part 4, Chapter 1 requirements must be met. These requirements include:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

------------------------------------------------------------------
                       COMBINATION PACKAGINGS 
------------------------------------------------------------------
                         |         |Inner      |Total    |Total
                         |  Inner  |packaging  |quantity |quantity
                         |packaging|quantity   |  per    |  per
UN number and proper     |  (see   | (per      |package -|package-
shipping name            |  6;3.2) |receptacle)|passenger| cargo
------------------------------------------------------------------
UN 1941 Dibromodifluoro- |  Glass  |  10.0 L   |         |
        methane          |---------------------|         |
                         | Plastics|  30.0 L   |  100 L  | 220 L
                         |---------------------|         |
                         |  Metal  |  40.0 L   |         |
------------------------------------------------------------------

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                        Drums                     Jerricans

Aluminium (4B)               Aluminium (1B1, 1B2)      Aluminium (3B1, 3B2)
Fibreboard (4G)              Fibre (1G)                Plastics (3H1, 3H2)
Natural wood (4C1, 4C2)      Other metal (1N1, 1N2)    Steel (3A1, 3A2)
Other metal (4N)             Plastics (1H1, 1H2)            
Plastics (4H1, 4H2)          Steel (1A1, 1A2)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)