Verpackungsanweisung 453 (für UN 2555)

Passenger aircraft for UN 2555 only

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

------------------------------------------------------------------------
COMBINATION PACKAGINGS
------------------------------------------------------------------------
                                | Inner     |Inner packaging|   Total
UN number and                   |packaging  |quantity (per  |  quantity
proper shipping name            |(see 6;3.2)| receptacle)   |per package
------------------------------------------------------------------------
UN 2555 Nitrocellulose          |   Glass   |    1.0 kg     |
        with water              |---------------------------|
                                |  Plastics |    1.0 kg     |
                                |---------------------------|   50 kg
                                |    Metal  |    1.0 kg     |
                                |---------------------------|
                                |Plastic bag|    1.0 kg     |
------------------------------------------------------------------------

ADDITIONAL PACKING REQUIREMENTS FOR COMBINATION PACKAGINGS

- Packagings must be designed and constructed to prevent the loss of water or alcohol content or the content of the phlegmatizer.

- Packagings must be so constructed and closed so as to avoid an explosive over pressure or pressure build-up of more than 300 kPa (3 bar).

OUTER PACKAGINGS OF COMBINATION PACKAGINGS (see 6;3.1)

Boxes                          Drums                      Jerricans

Aluminium (4B)                 Aluminium (1B2)            Aluminium (3B2)
Fibreboard (4G)                Fibre (1G)                 Other metal (3N2)
Natural wood (4C1, 4C2)        Other metal (1N2)          Plastics (3H1, 3H2)
Other metal (4N)               Plastics (1H1, 1H2)        Steel (3A2)
Plastics (4H1, 4H2)            Plywood (1D)
Plywood (4D)
Reconstituted wood (4F)
Steel (4A)