Verpackungsanweisung 872

Passenger and cargo aircraft für UN 2800

General requirements

Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

- Metal packagings must be corrosion resistant or be protected against corrosion.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

-----------------------------------------------------------------------
                  |                                 | Total   |  Total
                  |                                 | quantity|quantity
UN number and     |                                 |  per    |  per
proper            |                                 |package -|package
shipping name     | Packing conditions              |passenger|- cargo
-----------------------------------------------------------------------
UN 2800 Batteries,|Batteries must be protected      |         |
        wet, non- |against short circuits and must  |No limit |No limit
        spillable |be securely packed in strong     |         |
                  |outer packagings.                |         |
-----------------------------------------------------------------------

PACKAGINGS

Boxes                      Drums                       Jerricans

                   Strong outer packagings